**Chapter 24 Drycleaning**

24.1 General

24.1.1

Drycleaning plants shall comply with this chapter and NFPA 32.

24.1.2

Drycleaning plants or systems using solvents that have a flash point below 100°F (37.8°C) shall be prohibited.

24.2 Permits

Permits, where required, shall comply with Section 1.12.