**Chapter 2 Referenced Publications**

2.1 General

The documents or portions thereof listed in this chapter are referenced within this standard and shall be considered part of the requirements of this document.

2.2 NFPA Publications

National Fire Protection Association, 1 Batterymarch Park, Quincy, MA 02169-7471.

NFPA 13, Standard for the Installation of Sprinkler Systems, 2019 edition.

NFPA 70®, National Electrical Code®, 2017 edition.

NFPA 72®, National Fire Alarm and Signaling Code®, 2019 edition.

NFPA 220, Standard on Types of Building Construction, 2018 edition.

NFPA 750, Standard on Water Mist Fire Protection Systems, 2019 edition.

2.3 Other Publications

2.3.1 ASME Publications

American Society of Mechanical Engineers, Two Park Avenue, New York, NY 10016-5990.

ASME B16.1, Gray Iron Pipe Flanges and Flanged Fittings, Classes 25, 125, and 250, 2015.

ASME B16.3, Malleable Iron Threaded Fittings, Classes 150 and 300, 2016.

ASME B16.4, Gray Iron Threaded Fittings, Classes 125 and 250, 2016.

ASME B16.5, Pipe Flanges and Flanged Fittings, NPS 1/2 through NPS 24 Metric/Inch Standard, 2013.

ASME B16.9, Factory-Made Wrought Buttwelding Fittings, 2012.

ASME B16.11, Forged Fittings, Socket-Welding and Threaded, 2016.

ANSI/ASME B16.15, Cast Copper Alloy Threaded Fittings: Classes 125 and 250, 2013.

ASME B16.18, Cast Copper Alloy Solder Joint Pressure Fittings, 2012.

ASME B16.22, Wrought Copper and Copper Alloy Solder Joint Pressure Fittings, 2013.

ASME B16.25, Buttwelding Ends, 2012.

ASME B36.10M, Welded and Seamless Wrought Steel Pipe, 2015.

2.3.2 ASTM Publications

ASTM International, 100 Barr Harbor Drive, P.O. Box C700, West Conshohocken, PA 19428-2959.

ASTM A53/A53M, Standard Specification for Pipe, Steel, Black and Hot-Dipped, Zinc-Coated, Welded and Seamless, 2012.

ASTM A135/A135M, Standard Specification for Electric-Resistance-Welded Steel Pipe, 2009 (2014).

ASTM A234/A234M, Standard Specification for Piping Fittings of Wrought Carbon Steel and Alloy Steel for Moderate and High Temperature Service, 2016.

ASTM A795/A795M, Standard Specification for Black and Hot-Dipped Zinc-Coated (Galvanized) Welded and Seamless Steel Pipe for Fire Protection Use, 2013.

ASTM B32, Standard Specification for Solder Metal, 2008 (2014).

ASTM B43, Standard Specification for Seamless Red Brass Pipe, Standard Sizes, 2015.

ASTM B75/B75M, Standard Specification for Seamless Copper Tube, 2011.

ASTM B88, Standard Specification for Seamless Copper Water Tube, 2016.

ASTM B251, Standard Specification for General Requirements for Wrought Seamless Copper and Copper-Alloy Tube, 2010.

ASTM B813, Standard Specification for Liquid and Paste Fluxes for Soldering Applications of Copper and Copper-Alloy Tube, 2016.

ASTM B828, Standard Practice for Making Capillary Joints by Soldering of Copper and Copper Alloy Tube and Fittings, 2016.

ASTM F437, Standard Specification for Threaded Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe Fittings, Schedule 80, 2015.

ASTM F438, Standard Specification for Socket-Type Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe Fittings, Schedule 40, 2015.

ASTM F439, Standard Specification for Socket-Type Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe Fittings, Schedule 80, 2013.

ASTM F442/F442M, Standard Specification for Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Pipe (SDR-PR), 2013 el.

ASTM F876, Standard Specification for Crosslinked Polyethylene (PEX) Tubing, 2015a.

2.3.3 AWS Publications

American Welding Society, 8669 NW 36 Street, #130, Miami, FL 33166-6672.

AWS A5.8M/A5.8, Specification for Filler Metals for Brazing and Braze Welding, 2011.

2.3.4 Other Publications

Merriam-Webster's Collegiate Dictionary, 11th edition, Merriam-Webster, Inc., Springfield, MA, 2003.

2.4 References for Extracts in Mandatory Sections

NFPA 13R, Standard for the Installation of Sprinkler Systems in Low-Rise Residential Occupancies, 2019 edition.

NFPA 5000®, Building Construction and Safety Code®, 2018 edition.